(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A3")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 420 15)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GBR_CMD_Lower")
    )
  )

  (net 0 "")

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 064a777d-1941-4a0e-bfb2-9fa87d77752a)
    (at 85 44)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1cd759bc-b6a3-4f73-b53f-668a33c51009)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9be65664-d2d2-4bae-b676-c6cec9ed519c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ab09bb94-48c6-48c4-9609-1999e9217a68)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp c804f180-fd73-4720-a845-300a5935895e))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp f61cc391-1a7b-498b-8569-064a28c9a8e6))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp c6d509d0-ef65-44fd-9607-65d9d2347b39))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 1d468070-6d9f-4d0c-a01e-31ae4b2fcd87)
    (at 85.08 159)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1d788139-411a-403e-99f8-25a8d98add9b)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0a5843fe-9e27-4812-b54d-7cb5c78c7315)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0a4bb38c-4e0b-4167-801c-fc5ea5641a45)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 1bbf05b9-8fb9-4302-846d-6f029e6515fc))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp f46ddfcd-4696-40d8-9b3e-3db5685d51da))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 156fe247-53cf-4d51-93ef-b82fcc0e9a41))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 2c463cee-8e58-42ac-916b-484ab5d51d22)
    (at 230 44)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 37b73e2c-b240-406b-a094-4d05946aafc1)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 30a1d0dd-c388-453e-8564-2d0ff34d161b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 918974b9-df78-4d47-8182-9352cb384326)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp c340e3c2-6b87-4584-af76-936cab7cf4a6))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 59b28b7b-d88a-48ac-8d21-1b5775d3a8ea))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 79ca93bb-2db1-4c34-8ce4-969e4a88dba1))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 42487517-950b-4c74-9759-05ea87c75dac)
    (at 355 214)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e25bf9b9-2922-4108-9219-ac11037a6e9a)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 07d19561-b79c-4948-82a0-3ee75255eff2)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 67f0a80d-16ab-4a38-a031-cdbaa5ca1188)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 0b09318b-9cc7-466f-a83d-65adcfb826c6))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp d514d4b8-af74-402c-a866-74fa4e959ef0))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp ea97e68f-4bdd-42c7-ad65-4996d39393a0))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 4672601e-c80d-47c7-8a07-fe33387529ff)
    (at 355 239)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7abb869e-ffa5-4d2b-a9b3-7048c9b00c7f)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d40937f5-56b9-43d1-92ac-2b57ddf021c6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e0ef5f55-1c3b-4450-a711-9429087ce81c)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 5f1921ba-1223-496c-8a1f-1bd250adb512))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 8515f94b-045e-416e-ae70-34f9f1a9b31f))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 4b6b527c-58f7-46e7-86f2-2bf229810625))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 77660b36-9637-496f-b19c-93e11118da69)
    (at 230 29)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0755aee5-bc01-4cb5-b830-583289df50a3)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4a21e717-d46d-4d9e-8b98-af4ecb02d3ec)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec31c074-17b2-48e1-ab01-071acad3fa04)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 60dcd1fe-7079-4cb8-b509-04558ccf5097))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp c5eb1e4c-ce83-470e-8f32-e20ff1f886a3))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 9f8381e9-3077-4453-a480-a01ad9c1a940))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 7b68c2ce-a0dc-40af-9478-e4c008d437e2)
    (at 85 29)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d3d7e298-1d39-4294-a3ab-c84cc0dc5e5a)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 70e15522-1572-4451-9c0d-6d36ac70d8c6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dde51ae5-b215-445e-92bb-4a12ec410531)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 7599133e-c681-4202-85d9-c20dac196c64))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 4fb21471-41be-4be8-9687-66030f97befc))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp b96fe6ac-3535-4455-ab88-ed77f5e46d6e))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 812ee7e8-6898-482c-8612-52e7b7700a40)
    (at 355 29)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0755aee5-bc01-4cb5-b830-583289df50a3)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4a21e717-d46d-4d9e-8b98-af4ecb02d3ec)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec31c074-17b2-48e1-ab01-071acad3fa04)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 60dcd1fe-7079-4cb8-b509-04558ccf5097))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp c5eb1e4c-ce83-470e-8f32-e20ff1f886a3))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 9f8381e9-3077-4453-a480-a01ad9c1a940))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 84b18578-18bc-41f8-80dd-875cf8555c23)
    (at 230 159)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 97b6613c-3105-4b75-905c-fd4173eca018)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bfc838a4-cfb8-4f2f-843e-9d9cf0c4a0d6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec08f475-269c-40b8-bad4-dfa42ccc78a0)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 2b9f2d93-16e0-4458-9d28-ab4c309b5d35))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp f961c440-cfd1-47fe-b008-6315aaf626d0))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp ddc216f0-0507-49bb-831e-60415ce48a2a))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 8d0a8b35-d83c-48c3-8ede-c86f838ad516)
    (at 230 214)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e25bf9b9-2922-4108-9219-ac11037a6e9a)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 07d19561-b79c-4948-82a0-3ee75255eff2)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 67f0a80d-16ab-4a38-a031-cdbaa5ca1188)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 0b09318b-9cc7-466f-a83d-65adcfb826c6))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp d514d4b8-af74-402c-a866-74fa4e959ef0))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp ea97e68f-4bdd-42c7-ad65-4996d39393a0))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp 98fc9434-f13b-4492-b5e8-6140b01436c4)
    (at 355 44)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 37b73e2c-b240-406b-a094-4d05946aafc1)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 30a1d0dd-c388-453e-8564-2d0ff34d161b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 918974b9-df78-4d47-8182-9352cb384326)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp c340e3c2-6b87-4584-af76-936cab7cf4a6))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 59b28b7b-d88a-48ac-8d21-1b5775d3a8ea))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 79ca93bb-2db1-4c34-8ce4-969e4a88dba1))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp b533cd8c-a0ea-4e11-a4ee-db55a495b3f5)
    (at 85 214)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ca87f11b-5f48-4b57-8535-68d3ec2fe5a9)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7d928d56-093a-4ca8-aed1-414b7e703b45)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8a650ebf-3f78-4ca4-a26b-a5028693e36d)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 730b670c-9bcf-4dcd-9a8d-fcaa61fb0955))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp abe07c9a-17c3-43b5-b7a6-ae867ac27ea7))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 6d26d68f-1ca7-4ff3-b058-272f1c399047))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp b7433524-d569-4fc4-ac32-e83bf0b817e8)
    (at 355 159)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 97b6613c-3105-4b75-905c-fd4173eca018)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bfc838a4-cfb8-4f2f-843e-9d9cf0c4a0d6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec08f475-269c-40b8-bad4-dfa42ccc78a0)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 2b9f2d93-16e0-4458-9d28-ab4c309b5d35))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp f961c440-cfd1-47fe-b008-6315aaf626d0))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp ddc216f0-0507-49bb-831e-60415ce48a2a))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp c37210e2-d9ad-4677-a0d8-f45f8e5b2cd1)
    (at 230 239)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7abb869e-ffa5-4d2b-a9b3-7048c9b00c7f)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d40937f5-56b9-43d1-92ac-2b57ddf021c6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e0ef5f55-1c3b-4450-a711-9429087ce81c)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 5f1921ba-1223-496c-8a1f-1bd250adb512))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 8515f94b-045e-416e-ae70-34f9f1a9b31f))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 4b6b527c-58f7-46e7-86f2-2bf229810625))
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tstamp c583f65d-48d1-496d-8992-a53b91bb23ae)
    (at 85 239)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Fader_Board.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.8) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 85b7594c-358f-454b-b2ad-dd0b1d67ed76)
    )
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 16bd6381-8ac0-4bf2-9dce-ecc20c724b8d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a5cd8da1-8f7f-4f80-bb23-0317de562222)
    )
    (fp_circle (center 0 0) (end 2.8 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 4f66b314-0f62-4fb6-8c3c-f9c6a75cd3ec))
    (fp_circle (center 0 0) (end 3.05 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 01e9b6e7-adf9-4ee7-9447-a588630ee4a2))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 911bdcbe-493f-4e21-a506-7cbc636e2c17))
  )

  (gr_rect (start 235 34) (end 255 54)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 06c52b52-4abf-4654-bc63-6efec4e80df8))
  (gr_rect (start 95 124) (end 115 144)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 08ad29b6-4c82-44f8-91bc-cfcdbffdffe7))
  (gr_line (start 245 184) (end 245 204)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 08eda185-91bf-4dff-b183-e4879cfdf5ba))
  (gr_line (start 285 94) (end 285 34)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 0d407e41-1519-4d3d-b75c-1d834ad110fc))
  (gr_line (start 165 224) (end 145 224)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 1078b9e2-e2a3-4008-a3e1-ee305b37e225))
  (gr_line (start 165 204) (end 165 224)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 10e3904d-3292-4cd4-b212-c169509819bb))
  (gr_line (start 305 204) (end 305 184)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 1322fb93-c215-4429-ab7c-4522aff57f8a))
  (gr_line (start 285 184) (end 285 164)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 14d9ef1b-a5ab-4a93-8473-a415acecec18))
  (gr_line (start 285 204) (end 305 204)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 15041160-ac68-4ee2-adb7-3e8ac5de7482))
  (gr_rect (start 330 64) (end 350 84)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 283b22ca-c1d1-4e63-a177-66e71a7a01f9))
  (gr_line (start 285 224) (end 285 204)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 2d4201d9-97a8-452c-b87e-89c544b8ea21))
  (gr_line (start 265 224) (end 285 224)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 3517c94d-5a60-4c61-893d-eafb59391ab7))
  (gr_line (start 185 224) (end 185 204)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 37e69b7b-550b-4cd4-a5a3-635d8bbbb9c6))
  (gr_line (start 185 204) (end 165 204)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 3daaa4f8-3bd8-4c0b-95ac-10453ebca627))
  (gr_line (start 245 204) (end 265 204)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 3f293d94-863c-40b4-8b21-f8380fc05e8a))
  (gr_rect (start 235 64) (end 255 84)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 4aeb6170-61d2-4fe6-bd39-7d38f9e75627))
  (gr_rect (start 95 149) (end 115 169)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 4b69ef26-6273-4dfa-b63d-a377a9895b17))
  (gr_rect (start 95 174) (end 115 194)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 4f8fd8a6-7da3-4852-be5e-615d22213156))
  (gr_rect (start 235 124) (end 255 144)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 5718932d-daa2-497c-a753-09f3424c93c7))
  (gr_rect (start 235 94) (end 255 114)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 5c657cde-3136-4d25-a888-c67a5a00bb97))
  (gr_line (start 305 114) (end 305 94)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 5c8325ad-af0a-444c-862e-5e31838e8122))
  (gr_line (start 145 124) (end 225 124)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 62635d0e-ffb2-46ff-a74d-b6b63ca41b79))
  (gr_line (start 145 224) (end 145 124)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 6403546e-0743-49e1-9f6a-f16bdad5c3ec))
  (gr_rect (start 120 149) (end 140 169)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 66d6e3e9-f882-4e36-bca5-c0d75b48eff6))
  (gr_rect (start 80 24) (end 360 245)
    (stroke (width 0.1) (type solid)) (fill none) (layer "Edge.Cuts") (tstamp 68efda48-36c8-4efe-bd2d-73019cd33020))
  (gr_line (start 285 34) (end 265 34)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 78bbd21e-90f7-42d4-a673-58bdb9ae82e5))
  (gr_line (start 305 94) (end 285 94)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 7ae803c7-3bbf-435d-9e20-1f1e492c6810))
  (gr_line (start 225 224) (end 185 224)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 802d7c8d-99c6-4eb0-8893-4f13291dd0f8))
  (gr_line (start 265 204) (end 265 224)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 8ccc67e0-6516-4c0d-995c-9d9ba289fc51))
  (gr_line (start 265 114) (end 305 114)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp 967e641c-ab87-4fc3-8ea0-45a1fe4c1b23))
  (gr_rect (start 120 124) (end 140 144)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 9ece9ef3-de28-49e8-bb03-94fca3900b91))
  (gr_line (start 305 184) (end 285 184)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp b422d378-b702-433c-946a-d90c6afb49e9))
  (gr_rect (start 95 204) (end 115 224)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp b480d2ce-5be6-4230-a624-90a642f1ab9c))
  (gr_rect (start 265 124) (end 305 144)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp b6d3bc46-009a-4d12-a339-dae1e0441156))
  (gr_line (start 225 124) (end 225 224)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp c78ce1a0-27c0-485d-b5d4-6bf5cd0891b6))
  (gr_rect (start 165 34) (end 225 114)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp c7f11623-8c13-47cb-9b1b-c1aacfb1628f))
  (gr_line (start 265 34) (end 265 114)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp c8713c7e-237a-4a8c-8e57-921a7d41c58a))
  (gr_line (start 265 184) (end 245 184)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp cdab163f-f65d-4924-8a17-a9bd77d4b693))
  (gr_rect (start 290 34) (end 350 54)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp e019a420-f32b-4ff4-99a0-2dc4c9ab2422))
  (gr_rect (start 120 174) (end 140 194)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp e79f1fb7-1fec-4460-bb24-d1d35be65f00))
  (gr_rect (start 95 34) (end 155 114)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp eb87b1cf-81b3-413f-a61e-a4e599730af1))
  (gr_line (start 265 164) (end 265 184)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp edac32f8-f6b9-4636-8142-6c53faaa2ba4))
  (gr_line (start 285 164) (end 265 164)
    (stroke (width 0.1) (type default)) (layer "Edge.Cuts") (tstamp f5a92e9f-c23f-4cab-9fff-6bea31a906f6))
  (gr_rect (start 339 104) (end 341 183)
    (stroke (width 0.1) (type solid)) (fill none) (layer "Edge.Cuts") (tstamp fe78febf-411f-40d3-8c19-38c6f62a464a))

)
