Name       XXXXX;
Partno     XXXXX;
Date       XX/XX/XX;
Revision   XX;
Designer   XXXXX;
Company    XXXXX;
Assembly   XXXXX;
Location   XXXXX;
DEVICE g16v8a;

Pin 1 = IOREQ;
Pin 2 = RD;
Pin 3 = WR;

Pin 4 = A0;
Pin 5 = A1;
Pin 6 = A2;
Pin 7 = A3;
Pin 8 = A7;

Pin 19 = CRTC_CS;
Pin 18 = CRTC_RW;
Pin 17 = CRTC_E;

CRTC_CS = !(A7 & !IOREQ );
CRTC_RW = WR;
CRTC_E = !IOREQ;

