388787189753385
Package_DIP
DIP-4_W7.62mm
4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
4
4
Package_DIP
DIP-4_W7.62mm_LongPads
4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
4
4
Package_DIP
DIP-4_W7.62mm_SMDSocket_SmallPads
4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
4
4
Package_DIP
DIP-4_W7.62mm_Socket
4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
4
4
Package_DIP
DIP-4_W7.62mm_Socket_LongPads
4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
4
4
Package_DIP
DIP-4_W8.89mm_SMDSocket_LongPads
4-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
4
4
Package_DIP
DIP-4_W10.16mm
4-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
4
4
Package_DIP
DIP-4_W10.16mm_LongPads
4-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
4
4
Package_DIP
DIP-5-6_W7.62mm
5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
5
5
Package_DIP
DIP-5-6_W7.62mm_LongPads
5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
5
5
Package_DIP
DIP-5-6_W7.62mm_SMDSocket_SmallPads
5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
5
5
Package_DIP
DIP-5-6_W7.62mm_Socket
5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
5
5
Package_DIP
DIP-5-6_W7.62mm_Socket_LongPads
5-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
5
5
Package_DIP
DIP-5-6_W8.89mm_SMDSocket_LongPads
5-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
5
5
Package_DIP
DIP-5-6_W10.16mm
5-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
5
5
Package_DIP
DIP-5-6_W10.16mm_LongPads
5-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
5
5
Package_DIP
DIP-6_W7.62mm
6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
6
6
Package_DIP
DIP-6_W7.62mm_LongPads
6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
6
6
Package_DIP
DIP-6_W7.62mm_SMDSocket_SmallPads
6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
6
6
Package_DIP
DIP-6_W7.62mm_Socket
6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
6
6
Package_DIP
DIP-6_W7.62mm_Socket_LongPads
6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
6
6
Package_DIP
DIP-6_W8.89mm_SMDSocket_LongPads
6-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
6
6
Package_DIP
DIP-6_W10.16mm
6-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
6
6
Package_DIP
DIP-6_W10.16mm_LongPads
6-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
6
6
Package_DIP
DIP-8-16_W7.62mm
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
8
8
Package_DIP
DIP-8-16_W7.62mm_Socket
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
8
8
Package_DIP
DIP-8-16_W7.62mm_Socket_LongPads
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
8
8
Package_DIP
DIP-8-N6_W7.62mm
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), missing pin 6
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
7
7
Package_DIP
DIP-8-N7_W7.62mm
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), missing pin 7
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
7
7
Package_DIP
DIP-8_W7.62mm
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
8
8
Package_DIP
DIP-8_W7.62mm_LongPads
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
8
8
Package_DIP
DIP-8_W7.62mm_SMDSocket_SmallPads
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
8
8
Package_DIP
DIP-8_W7.62mm_Socket
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
8
8
Package_DIP
DIP-8_W7.62mm_Socket_LongPads
8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
8
8
Package_DIP
DIP-8_W8.89mm_SMDSocket_LongPads
8-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
8
8
Package_DIP
DIP-8_W10.16mm
8-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
8
8
Package_DIP
DIP-8_W10.16mm_LongPads
8-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
8
8
Package_DIP
DIP-10_W7.62mm
10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
10
10
Package_DIP
DIP-10_W7.62mm_LongPads
10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
10
10
Package_DIP
DIP-10_W7.62mm_SMDSocket_SmallPads
10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
10
10
Package_DIP
DIP-10_W7.62mm_Socket
10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
10
10
Package_DIP
DIP-10_W7.62mm_Socket_LongPads
10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
10
10
Package_DIP
DIP-10_W8.89mm_SMDSocket_LongPads
10-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
10
10
Package_DIP
DIP-10_W10.16mm
10-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
10
10
Package_DIP
DIP-10_W10.16mm_LongPads
10-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
10
10
Package_DIP
DIP-12_W7.62mm
12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
12
12
Package_DIP
DIP-12_W7.62mm_LongPads
12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
12
12
Package_DIP
DIP-12_W7.62mm_SMDSocket_SmallPads
12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
12
12
Package_DIP
DIP-12_W7.62mm_Socket
12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
12
12
Package_DIP
DIP-12_W7.62mm_Socket_LongPads
12-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
12
12
Package_DIP
DIP-12_W8.89mm_SMDSocket_LongPads
12-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
12
12
Package_DIP
DIP-12_W10.16mm
12-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
12
12
Package_DIP
DIP-12_W10.16mm_LongPads
12-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
12
12
Package_DIP
DIP-14_W7.62mm
14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
14
14
Package_DIP
DIP-14_W7.62mm_LongPads
14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
14
14
Package_DIP
DIP-14_W7.62mm_SMDSocket_SmallPads
14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
14
14
Package_DIP
DIP-14_W7.62mm_Socket
14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
14
14
Package_DIP
DIP-14_W7.62mm_Socket_LongPads
14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
14
14
Package_DIP
DIP-14_W8.89mm_SMDSocket_LongPads
14-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
14
14
Package_DIP
DIP-14_W10.16mm
14-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
14
14
Package_DIP
DIP-14_W10.16mm_LongPads
14-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
14
14
Package_DIP
DIP-16_W7.62mm
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
16
16
Package_DIP
DIP-16_W7.62mm_LongPads
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
16
16
Package_DIP
DIP-16_W7.62mm_SMDSocket_SmallPads
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
16
16
Package_DIP
DIP-16_W7.62mm_Socket
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
16
16
Package_DIP
DIP-16_W7.62mm_Socket_LongPads
16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
16
16
Package_DIP
DIP-16_W8.89mm_SMDSocket_LongPads
16-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
16
16
Package_DIP
DIP-16_W10.16mm
16-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
16
16
Package_DIP
DIP-16_W10.16mm_LongPads
16-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
16
16
Package_DIP
DIP-18_W7.62mm
18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
18
18
Package_DIP
DIP-18_W7.62mm_LongPads
18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
18
18
Package_DIP
DIP-18_W7.62mm_SMDSocket_SmallPads
18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
18
18
Package_DIP
DIP-18_W7.62mm_Socket
18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
18
18
Package_DIP
DIP-18_W7.62mm_Socket_LongPads
18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
18
18
Package_DIP
DIP-18_W8.89mm_SMDSocket_LongPads
18-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
18
18
Package_DIP
DIP-20_W7.62mm
20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
20
20
Package_DIP
DIP-20_W7.62mm_LongPads
20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
20
20
Package_DIP
DIP-20_W7.62mm_SMDSocket_SmallPads
20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
20
20
Package_DIP
DIP-20_W7.62mm_Socket
20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
20
20
Package_DIP
DIP-20_W7.62mm_Socket_LongPads
20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
20
20
Package_DIP
DIP-20_W8.89mm_SMDSocket_LongPads
20-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
20
20
Package_DIP
DIP-22_W7.62mm
22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
22
22
Package_DIP
DIP-22_W7.62mm_LongPads
22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
22
22
Package_DIP
DIP-22_W7.62mm_SMDSocket_SmallPads
22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
22
22
Package_DIP
DIP-22_W7.62mm_Socket
22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
22
22
Package_DIP
DIP-22_W7.62mm_Socket_LongPads
22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
22
22
Package_DIP
DIP-22_W8.89mm_SMDSocket_LongPads
22-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
22
22
Package_DIP
DIP-22_W10.16mm
22-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
22
22
Package_DIP
DIP-22_W10.16mm_LongPads
22-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
22
22
Package_DIP
DIP-22_W10.16mm_SMDSocket_SmallPads
22-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil SMDSocket SmallPads
0
22
22
Package_DIP
DIP-22_W10.16mm_Socket
22-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), Socket
THT DIP DIL PDIP 2.54mm 10.16mm 400mil Socket
0
22
22
Package_DIP
DIP-22_W10.16mm_Socket_LongPads
22-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil Socket LongPads
0
22
22
Package_DIP
DIP-22_W11.43mm_SMDSocket_LongPads
22-lead though-hole mounted DIP package, row spacing 11.43 mm (450 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 11.43mm 450mil SMDSocket LongPads
0
22
22
Package_DIP
DIP-24_W7.62mm
24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
24
24
Package_DIP
DIP-24_W7.62mm_LongPads
24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
24
24
Package_DIP
DIP-24_W7.62mm_SMDSocket_SmallPads
24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
24
24
Package_DIP
DIP-24_W7.62mm_Socket
24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
24
24
Package_DIP
DIP-24_W7.62mm_Socket_LongPads
24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
24
24
Package_DIP
DIP-24_W8.89mm_SMDSocket_LongPads
24-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
24
24
Package_DIP
DIP-24_W10.16mm
24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)
THT DIP DIL PDIP 2.54mm 10.16mm 400mil
0
24
24
Package_DIP
DIP-24_W10.16mm_LongPads
24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil LongPads
0
24
24
Package_DIP
DIP-24_W10.16mm_SMDSocket_SmallPads
24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil SMDSocket SmallPads
0
24
24
Package_DIP
DIP-24_W10.16mm_Socket
24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), Socket
THT DIP DIL PDIP 2.54mm 10.16mm 400mil Socket
0
24
24
Package_DIP
DIP-24_W10.16mm_Socket_LongPads
24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 10.16mm 400mil Socket LongPads
0
24
24
Package_DIP
DIP-24_W11.43mm_SMDSocket_LongPads
24-lead though-hole mounted DIP package, row spacing 11.43 mm (450 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 11.43mm 450mil SMDSocket LongPads
0
24
24
Package_DIP
DIP-24_W15.24mm
24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
24
24
Package_DIP
DIP-24_W15.24mm_LongPads
24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
24
24
Package_DIP
DIP-24_W15.24mm_SMDSocket_SmallPads
24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
24
24
Package_DIP
DIP-24_W15.24mm_Socket
24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
24
24
Package_DIP
DIP-24_W15.24mm_Socket_LongPads
24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
24
24
Package_DIP
DIP-24_W16.51mm_SMDSocket_LongPads
24-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
24
24
Package_DIP
DIP-28_W7.62mm
28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
28
28
Package_DIP
DIP-28_W7.62mm_LongPads
28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
28
28
Package_DIP
DIP-28_W7.62mm_SMDSocket_SmallPads
28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil SMDSocket SmallPads
0
28
28
Package_DIP
DIP-28_W7.62mm_Socket
28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket
0
28
28
Package_DIP
DIP-28_W7.62mm_Socket_LongPads
28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads
0
28
28
Package_DIP
DIP-28_W8.89mm_SMDSocket_LongPads
28-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads
0
28
28
Package_DIP
DIP-28_W15.24mm
28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
28
28
Package_DIP
DIP-28_W15.24mm_LongPads
28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
28
28
Package_DIP
DIP-28_W15.24mm_SMDSocket_SmallPads
28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
28
28
Package_DIP
DIP-28_W15.24mm_Socket
28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
28
28
Package_DIP
DIP-28_W15.24mm_Socket_LongPads
28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
28
28
Package_DIP
DIP-28_W16.51mm_SMDSocket_LongPads
28-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
28
28
Package_DIP
DIP-32_W7.62mm
32-lead dip package, row spacing 7.62 mm (300 mils)
DIL DIP PDIP 2.54mm 7.62mm 300mil
0
32
32
Package_DIP
DIP-32_W15.24mm
32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
32
32
Package_DIP
DIP-32_W15.24mm_LongPads
32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
32
32
Package_DIP
DIP-32_W15.24mm_SMDSocket_SmallPads
32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
32
32
Package_DIP
DIP-32_W15.24mm_Socket
32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
32
32
Package_DIP
DIP-32_W15.24mm_Socket_LongPads
32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
32
32
Package_DIP
DIP-32_W16.51mm_SMDSocket_LongPads
32-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
32
32
Package_DIP
DIP-40_W15.24mm
40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
40
40
Package_DIP
DIP-40_W15.24mm_LongPads
40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
40
40
Package_DIP
DIP-40_W15.24mm_SMDSocket_SmallPads
40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
40
40
Package_DIP
DIP-40_W15.24mm_Socket
40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
40
40
Package_DIP
DIP-40_W15.24mm_Socket_LongPads
40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
40
40
Package_DIP
DIP-40_W16.51mm_SMDSocket_LongPads
40-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
40
40
Package_DIP
DIP-40_W25.4mm
40-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils)
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil
0
40
40
Package_DIP
DIP-40_W25.4mm_LongPads
40-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), LongPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil LongPads
0
40
40
Package_DIP
DIP-40_W25.4mm_SMDSocket_SmallPads
40-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil SMDSocket SmallPads
0
40
40
Package_DIP
DIP-40_W25.4mm_Socket
40-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), Socket
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil Socket
0
40
40
Package_DIP
DIP-40_W25.4mm_Socket_LongPads
40-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil Socket LongPads
0
40
40
Package_DIP
DIP-40_W26.67mm_SMDSocket_LongPads
40-lead though-hole mounted DIP package, row spacing 26.67 mm (1050 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 26.669999999999998mm 1050mil SMDSocket LongPads
0
40
40
Package_DIP
DIP-42_W15.24mm
42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
42
42
Package_DIP
DIP-42_W15.24mm_LongPads
42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
42
42
Package_DIP
DIP-42_W15.24mm_SMDSocket_SmallPads
42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
42
42
Package_DIP
DIP-42_W15.24mm_Socket
42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
42
42
Package_DIP
DIP-42_W15.24mm_Socket_LongPads
42-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
42
42
Package_DIP
DIP-42_W16.51mm_SMDSocket_LongPads
42-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
42
42
Package_DIP
DIP-48_W15.24mm
48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
48
48
Package_DIP
DIP-48_W15.24mm_LongPads
48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
48
48
Package_DIP
DIP-48_W15.24mm_SMDSocket_SmallPads
48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
48
48
Package_DIP
DIP-48_W15.24mm_Socket
48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
48
48
Package_DIP
DIP-48_W15.24mm_Socket_LongPads
48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
48
48
Package_DIP
DIP-48_W16.51mm_SMDSocket_LongPads
48-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
48
48
Package_DIP
DIP-64_W15.24mm
64-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)
THT DIP DIL PDIP 2.54mm 15.24mm 600mil
0
64
64
Package_DIP
DIP-64_W15.24mm_LongPads
64-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads
0
64
64
Package_DIP
DIP-64_W15.24mm_SMDSocket_SmallPads
64-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil SMDSocket SmallPads
0
64
64
Package_DIP
DIP-64_W15.24mm_Socket
64-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket
0
64
64
Package_DIP
DIP-64_W15.24mm_Socket_LongPads
64-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads
0
64
64
Package_DIP
DIP-64_W16.51mm_SMDSocket_LongPads
64-lead though-hole mounted DIP package, row spacing 16.51 mm (650 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 16.51mm 650mil SMDSocket LongPads
0
64
64
Package_DIP
DIP-64_W22.86mm
64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils)
THT DIP DIL PDIP 2.54mm 22.86mm 900mil
0
64
64
Package_DIP
DIP-64_W22.86mm_LongPads
64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils), LongPads
THT DIP DIL PDIP 2.54mm 22.86mm 900mil LongPads
0
64
64
Package_DIP
DIP-64_W22.86mm_SMDSocket_SmallPads
64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 22.86mm 900mil SMDSocket SmallPads
0
64
64
Package_DIP
DIP-64_W22.86mm_Socket
64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils), Socket
THT DIP DIL PDIP 2.54mm 22.86mm 900mil Socket
0
64
64
Package_DIP
DIP-64_W22.86mm_Socket_LongPads
64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 22.86mm 900mil Socket LongPads
0
64
64
Package_DIP
DIP-64_W24.13mm_SMDSocket_LongPads
64-lead though-hole mounted DIP package, row spacing 24.13 mm (950 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 24.13mm 950mil SMDSocket LongPads
0
64
64
Package_DIP
DIP-64_W25.4mm
64-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils)
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil
0
64
64
Package_DIP
DIP-64_W25.4mm_LongPads
64-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), LongPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil LongPads
0
64
64
Package_DIP
DIP-64_W25.4mm_SMDSocket_SmallPads
64-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), SMDSocket, SmallPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil SMDSocket SmallPads
0
64
64
Package_DIP
DIP-64_W25.4mm_Socket
64-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), Socket
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil Socket
0
64
64
Package_DIP
DIP-64_W25.4mm_Socket_LongPads
64-lead though-hole mounted DIP package, row spacing 25.4 mm (1000 mils), Socket, LongPads
THT DIP DIL PDIP 2.54mm 25.4mm 1000mil Socket LongPads
0
64
64
Package_DIP
DIP-64_W26.67mm_SMDSocket_LongPads
64-lead though-hole mounted DIP package, row spacing 26.67 mm (1050 mils), SMDSocket, LongPads
THT DIP DIL PDIP 2.54mm 26.669999999999998mm 1050mil SMDSocket LongPads
0
64
64
Package_DIP
Fairchild_LSOP-8
8-Lead, 300\" Wide, Surface Mount Package (https://www.fairchildsemi.com/package-drawings/ML/MLSOP08A.pdf)
LSOP 2.54mm 300mil
0
8
8
Package_DIP
PowerIntegrations_PDIP-8B
Power Integrations variant of 8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads, see https://www.power.com/sites/default/files/product-docs/lnk520.pdf
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
7
7
Package_DIP
PowerIntegrations_PDIP-8C
Power Integrations variant of 8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads, see https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-iii_family_datasheet.pdf
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
7
7
Package_DIP
PowerIntegrations_SDIP-10C
PowerIntegrations variant of 10-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads, see https://www.power.com/sites/default/files/product-docs/tophx_family_datasheet.pdf
THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads
0
9
9
Package_DIP
PowerIntegrations_SMD-8
PowerIntegrations variant of 8-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils), see https://www.power.com/sites/default/files/product-docs/lnk520.pdf
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
8
8
Package_DIP
PowerIntegrations_SMD-8B
PowerIntegrations variant of 8-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils), see https://www.power.com/sites/default/files/product-docs/lnk520.pdf
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
7
7
Package_DIP
PowerIntegrations_SMD-8C
PowerIntegrations variant of 8-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils), see https://ac-dc.power.com/sites/default/files/product-docs/tinyswitch-iii_family_datasheet.pdf
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
7
7
Package_DIP
PowerIntegrations_eDIP-12B
Power Integrations eDIP-12B, see https://www.power.com/sites/default/files/product-docs/linkswitch-pl_family_datasheet.pdf
THT DIP DIL PDIP 2.54mm 7.62mm 300mil
0
11
11
Package_DIP
SMDIP-4_W7.62mm
4-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
4
4
Package_DIP
SMDIP-4_W9.53mm
4-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
4
4
Package_DIP
SMDIP-4_W9.53mm_Clearance8mm
4-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
4
4
Package_DIP
SMDIP-4_W11.48mm
4-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
4
4
Package_DIP
SMDIP-6_W7.62mm
6-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
6
6
Package_DIP
SMDIP-6_W9.53mm
6-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
6
6
Package_DIP
SMDIP-6_W9.53mm_Clearance8mm
6-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
6
6
Package_DIP
SMDIP-6_W11.48mm
6-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
6
6
Package_DIP
SMDIP-8_W7.62mm
8-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
8
8
Package_DIP
SMDIP-8_W9.53mm
8-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
8
8
Package_DIP
SMDIP-8_W9.53mm_Clearance8mm
8-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
8
8
Package_DIP
SMDIP-8_W11.48mm
8-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
8
8
Package_DIP
SMDIP-10_W7.62mm
10-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
10
10
Package_DIP
SMDIP-10_W9.53mm
10-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
10
10
Package_DIP
SMDIP-10_W9.53mm_Clearance8mm
10-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
10
10
Package_DIP
SMDIP-10_W11.48mm
10-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
10
10
Package_DIP
SMDIP-12_W7.62mm
12-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
12
12
Package_DIP
SMDIP-12_W9.53mm
12-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
12
12
Package_DIP
SMDIP-12_W9.53mm_Clearance8mm
12-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
12
12
Package_DIP
SMDIP-12_W11.48mm
12-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
12
12
Package_DIP
SMDIP-14_W7.62mm
14-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
14
14
Package_DIP
SMDIP-14_W9.53mm
14-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
14
14
Package_DIP
SMDIP-14_W9.53mm_Clearance8mm
14-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
14
14
Package_DIP
SMDIP-14_W11.48mm
14-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
14
14
Package_DIP
SMDIP-16_W7.62mm
16-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
16
16
Package_DIP
SMDIP-16_W9.53mm
16-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
16
16
Package_DIP
SMDIP-16_W9.53mm_Clearance8mm
16-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
16
16
Package_DIP
SMDIP-16_W11.48mm
16-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
16
16
Package_DIP
SMDIP-18_W7.62mm
18-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
18
18
Package_DIP
SMDIP-18_W9.53mm
18-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
18
18
Package_DIP
SMDIP-18_W9.53mm_Clearance8mm
18-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
18
18
Package_DIP
SMDIP-18_W11.48mm
18-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
18
18
Package_DIP
SMDIP-20_W7.62mm
20-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
20
20
Package_DIP
SMDIP-20_W9.53mm
20-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
20
20
Package_DIP
SMDIP-20_W9.53mm_Clearance8mm
20-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
20
20
Package_DIP
SMDIP-20_W11.48mm
20-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
20
20
Package_DIP
SMDIP-22_W7.62mm
22-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
22
22
Package_DIP
SMDIP-22_W9.53mm
22-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
22
22
Package_DIP
SMDIP-22_W9.53mm_Clearance8mm
22-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm
0
22
22
Package_DIP
SMDIP-22_W11.48mm
22-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
22
22
Package_DIP
SMDIP-24_W7.62mm
24-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
24
24
Package_DIP
SMDIP-24_W9.53mm
24-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
24
24
Package_DIP
SMDIP-24_W11.48mm
24-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
24
24
Package_DIP
SMDIP-24_W15.24mm
24-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
24
24
Package_DIP
SMDIP-28_W15.24mm
28-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
28
28
Package_DIP
SMDIP-32_W7.62mm
32-lead surface-mounted (SMD) DIP package, row spacing 7.62 mm (300 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 7.62mm 300mil
0
32
32
Package_DIP
SMDIP-32_W9.53mm
32-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil
0
32
32
Package_DIP
SMDIP-32_W11.48mm
32-lead surface-mounted (SMD) DIP package, row spacing 11.48 mm (451 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 11.48mm 451mil
0
32
32
Package_DIP
SMDIP-32_W15.24mm
32-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
32
32
Package_DIP
SMDIP-40_W15.24mm
40-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
40
40
Package_DIP
SMDIP-40_W25.24mm
40-lead surface-mounted (SMD) DIP package, row spacing 25.24 mm (993 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 25.24mm 993mil
0
40
40
Package_DIP
SMDIP-42_W15.24mm
42-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
42
42
Package_DIP
SMDIP-48_W15.24mm
48-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
48
48
Package_DIP
SMDIP-64_W15.24mm
64-lead surface-mounted (SMD) DIP package, row spacing 15.24 mm (600 mils)
SMD DIP DIL PDIP SMDIP 2.54mm 15.24mm 600mil
0
64
64
Package_DIP
Toshiba_11-7A9
Toshiba 11-7A9 package, like 6-lead dip package with missing pin 5, row spacing 7.62 mm (300 mils), https://toshiba.semicon-storage.com/info/docget.jsp?did=1421&prodName=TLP3021(S)
Toshiba 11-7A9 DIL DIP PDIP 2.54mm 7.62mm 300mil
0
5
5
Package_DIP
Vishay_HVM-DIP-3_W7.62mm
3-lead though-hole mounted high-volatge DIP package (based on standard DIP-4), row spacing 7.62 mm (300 mils), see https://www.vishay.com/docs/91361/hexdip.pdf
THT DIP DIL PDIP 2.54mm 7.62mm 300mil Vishay HVMDIP HEXDIP
0
4
3
